For critical applications, dryer can be designed to reduce exiting dew point to -80°F (-62°C). Dryer cycle is based on 4 minute cycle. Repressurization circuit is added to ensure full repressurization at switchover. Includes adjustable purge and pressure relief valves. Note that there is a reduced flow capacity with this option. Moisture Load Control not available. Contact Factory for recommendations.