A single flange connection is provided after the air leaves the moisture separators and a single flange connection is provided to enter the reheater vessel. Does not include the filter or interconnecting piping. May be used with either HDF Mist Eliminator or flanged filter. Consult factory for dimensions.