* Prepiped coalescing filter with automatic drain installed
* Prepiped particulate afterfilter
* Pressure differential indicators on both filters.
* Three valve dryer bypass