* Prepiped coalescing prefilter with automatic drain installed
* Prepiped particulate afterfilter
* Three valve bypasses around pre and afterfilter
* Pressure differential indicators on both filters.