90ZPB-1500ZPB

* Prepiped particulate prefilter (grade G) with automatic drain installed
* Prepiped coalescing prefilter (grade H) with automatic drain installed
* Prepiped particulate afterfilter (grade G)
* Three valve bypasses around pre and afterfilters and dryer bypass
* Pressure differential indicators on all filters

1800ZPB-5000ZPB

* Skid Mounted particulate prefilter (grade G) with manual drain valve installed
* Skid Mounted coalescing prefilter (grade H) with manual drain valve installed
* Skid Mounted particulate afterfilter (grade G)
* Three valve bypasses around pre and afterfilter and dryer bypass
* Pressure differential indicators on all filters.