Provides high accuracy monitoring of the dryers performance. Should a high humidity alarm condition exist in the outlet air stream of the dryer, the alarm condition is communicated through the DPC Controller to signal the need for system service.