Intended for indoor or outdoor installation where a degree of protection is required from rain or sleet or falling water (such as a sprinkler). Application ambient temperature must not be below 45⁰F.