Pneumatically operated zero air loss demand drain with isolation valves for ease in cleaning. Includes liquid level switch that communicates drain malfunction to controller.