Automatically monitors tower pressure for proper sequencing and operation of valves. Should the valve be out of position during the cycle, a visual alarm will be activated to alert maintenance personnel.