Field Installed Gauge Assembly provided.

Assembly includes (1) Pressure (0-300 PSIG) and (1) Temperature (0-160°F) Gauge.

Note: (2) Gauge Assemblies are required to measure both Inlet and Outlet conditions. Suction Pressure Gauge standard on 75-150 models.