**-80°F Dew Point**

For critical applications dryer can be designed to reduce exiting dew point to -80°F (-62°C). Dryer cycle is based on a 4 minute cycle. A repressurization circuit is added to ensure full repressuriztion at switchover. Note that there is a reduced flow capacity with this option.Standard Moisture Load Control w/ Fail to Shift is not available. Requires Moisture Load Control w/Dew Point Display option.