Allows for manual purge adjustment based on the inlet flow and pressure.