Coalescing filter is mounted between the chiller system and the reheat system. Includes insulation and separate drain for the filter. Provides high efficiency filtration at coldest point in system for superior contaminant removal.