Enhanced controller that monitors air inlet pressure and temperature and outlet air pressure and temperature in addition to the display and operating parameters on the standard controller. Includes Remote Stop / Start functionality.

Microprocessor shall also incorporate field programmable chiller temperature settings to allow the dryer more closely match to seasonal demands. A higher chiller temperature setting shall allow the refrigerant compressors to experience a lighter load thereby conserving more energy and further reducing compressor wear and tear.