90ZPB-1500ZPB

* Prepiped particulate prefilter (grade H) with automatic drain installed.
* Prepiped particulate afterfilter (grade G)
* Pressure differential indicators on both filters

1800ZPB-5000ZPB

* Ship Loose coalescing prefilter (grade H)
* Ship Loose particulate afterfilter (grade G)
* Pressure differential indicators on both filters