Accurately monitors humidity levels of the compressed air. Should a malfunction occur and a high humidity condition exist; a visual alarm will be activated to alert maintenance personnel.