Prevents direct contact with hot vessel surfaces while increasing regeneration efficiency.