**NEMA 4/DPC Option (Includes the following):**

***NEMA 4 Electrical Enclosure***

NEMA 4 enclosures protect enclosed equipment against water, seepage of water, falling or hose directed water and severe external condensation. NEMA 4 enclosures are suitable for indoors and outdoors use.

***Digital Controller***

Programmable Logic Controller with graphical interface, backlit display, MODBUS communications via RS-485 and maintenance reminders. Digital Controller Includes:

* SelectDry™ feature which permits selectable dew point operation, allowing the user to select the outlet pressure dew point from -40 or -4°F.
* *PurgeSync*™ enables dryer operation to “mirror” that of the main air compressor. When the air compressor either unloads or is turned off, *PurgeSync*™ automatically completes the current drying cycle and closes the purge valves until the compressor indicates the need for more air. Allows dryer to use purge air from downstream storage, reducing compressor cycling when air demand is low.

***DynOptic™ Panel***

Provides visual indication of dryer status. Includes LED indicators for:

* Dryer On / Alarm
* Left / Right Tower Drying
* Left / Right Tower Regenerating

***UL / ULC Panel***

Electrical panel listed to UL 508A.