**-100 °F Dew Point**

For critical applications, dryer can be designed to reduce exiting dew point to -100°F (-73°C). Dryer cycle is based on 4 minute cycle. A repressurization circuit is added to ensure full repressurization at switchover. Includes adjustable purge and pressure relief valves. Note that there is a reduced flow capacity with this option. Standard Moisture Load Control w/ Fail to Shift is not available. Contact Factory for recommendations.