90ZPB-1500ZPB

* Prepiped coalescing prefilter (grade H) with automatic drain installed
* Prepiped particulate afterfilter (grade G)
* Pressure differential indicators on both filters
* Three valve dryer bypass

1800ZPB-5000ZPB

* Skid Mounted coalescing prefilter (grade H) with manual drain valve installed
* Skid Mounted particulate afterfilter (grade G)
* Pressure differential indicators on both filters
* Three valve dryer bypass