NEMA 4/DPC option provides increased protection of electrical components with enhanced controls and displays. This package includes the following:

Digital Controller: PLC programmable controller with integral keypad and backlit display.

NEMA 4 Electrical Enclosure: Protects electrical components from rain or hose directed water. Suitable for outdoor installations.

UL/ULC electrical Panel: Electrical panel constructed in accordance with UL/ULC 508A.

DynOptic™ Panel: Provides visual indication of dryer status. Includes LED indicators for Tower Drying, Tower Regenerating, Power On and Power Off / Alarm.