Provides continuous monitoring of dryer discharge air temperature. Should a high outlet temperature exist, an alarm is activated to alert service personnel of alarm condition.