The Power Saver feature provides temperature sensing of the outlet purge air stream. When the purge air temperature indicates that the tower

regeneration has been completed, the heater is turned off, thus saving valuable regeneration energy. Especially effective during times of low moisture loading, such as when low air flow requirements exist or during dry winter months.