Electronic microprocessor-controlled drain has large internal orifices for reliable removal of condensate. Drain kit shipped separately for field installation on 75-150 SCFM models.