Type 4 enclosures are intended to protect the equipment against splashing water, seepage of water, falling or hose-directed water and severe external condensation.