The Microprocessor Controller is configured with MODBUS capabilities. MODBUS enables the user to establish master-slave communications with any connected device that supports the MODBUS protocol. The controller currently supports MODBUS TCP/IP.