90ZPB-1500ZPB

* Prepiped particulate prefilter (grade G) with automatic drain installed
* Prepiped coalescing prefilter (grade H) with automatic drain installed
* Prepiped particulate afterfilter (grade G)
* Pressure differential indicators on all filters

1800ZPB-5000ZPB

* Ship Loose particulate prefilter (grade G)
* Ship Loose coalescing prefilter (grade H)
* Ship Loose particulate afterfilter (grade G)
* Pressure differential indicators on all filters