Replaces standard solid state timer with pneumatically operated timer. Note that no electrical options are available with the pneumatic controls option. Unit meets NEMA 7 classification.